Qt 4.6: receiver.cpp Example File (network/broadcastreceiver/receiver.cpp)

|  | Home · All Classes · Overviews |

# receiver.cpp Example File
network/broadcastreceiver/receiver.cpp

     /****************************************************************************
     **
     ** Copyright (C) 2009 Nokia Corporation and/or its subsidiary(-ies).
     ** Contact: Nokia Corporation (qt-info@nokia.com)
     **
     ** This file is part of the examples of the Qt Toolkit.
     **
     ** $QT_BEGIN_LICENSE:LGPL$
     ** No Commercial Usage
     ** This file contains pre-release code and may not be distributed.
     ** You may use this file in accordance with the terms and conditions
     ** contained in the Technology Preview License Agreement accompanying
     ** this package.
     **
     ** GNU Lesser General Public License Usage
     ** Alternatively, this file may be used under the terms of the GNU Lesser
     ** General Public License version 2.1 as published by the Free Software
     ** Foundation and appearing in the file LICENSE.LGPL included in the
     ** packaging of this file.  Please review the following information to
     ** ensure the GNU Lesser General Public License version 2.1 requirements
     ** will be met: http://www.gnu.org/licenses/old-licenses/lgpl-2.1.html.
     **
     ** In addition, as a special exception, Nokia gives you certain
     ** additional rights.  These rights are described in the Nokia Qt LGPL
     ** Exception version 1.1, included in the file LGPL_EXCEPTION.txt in this
     ** package.
     **
     ** If you have questions regarding the use of this file, please contact
     ** Nokia at qt-info@nokia.com.
     **
     **
     **
     **
     **
     **
     **
     **
     ** $QT_END_LICENSE$
     **
     ****************************************************************************/

     #include <QtGui>
     #include <QtNetwork>

     #include "receiver.h"

     Receiver::Receiver(QWidget *parent)
         : QDialog(parent)
     {
         statusLabel = new QLabel(tr("Listening for broadcasted messages"));
         quitButton = new QPushButton(tr("&Quit"));

         udpSocket = new QUdpSocket(this);
         udpSocket->bind(45454);

         connect(udpSocket, SIGNAL(readyRead()),
                 this, SLOT(processPendingDatagrams()));
         connect(quitButton, SIGNAL(clicked()), this, SLOT(close()));

         QHBoxLayout *buttonLayout = new QHBoxLayout;
         buttonLayout->addStretch(1);
         buttonLayout->addWidget(quitButton);
         buttonLayout->addStretch(1);

         QVBoxLayout *mainLayout = new QVBoxLayout;
         mainLayout->addWidget(statusLabel);
         mainLayout->addLayout(buttonLayout);
         setLayout(mainLayout);

         setWindowTitle(tr("Broadcast Receiver"));
     }

     void Receiver::processPendingDatagrams()
     {
         while (udpSocket->hasPendingDatagrams()) {
             QByteArray datagram;
             datagram.resize(udpSocket->pendingDatagramSize());
             udpSocket->readDatagram(datagram.data(), datagram.size());
             statusLabel->setText(tr("Received datagram: \"%1\"")
                                  .arg(datagram.data()));
         }
     }